#MicroXplorer Configuration settings - do not modify
ADC1.Channel-1\#ChannelRegularConversion=ADC_CHANNEL_3
ADC1.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_6
ADC1.Channel-3\#ChannelRegularConversion=ADC_CHANNEL_7
ADC1.ClockPrescaler=ADC_CLOCK_ASYNC_DIV4
ADC1.CommonPathInternal=null|null|null|null
ADC1.ContinuousConvMode=ENABLE
ADC1.DMAContinuousRequests=ENABLE
ADC1.EOCSelection=ADC_EOC_SEQ_CONV
ADC1.ExternalTrigConv=ADC_SOFTWARE_START
ADC1.IPParameters=Rank-1\#ChannelRegularConversion,Channel-1\#ChannelRegularConversion,SamplingTime-1\#ChannelRegularConversion,OffsetNumber-1\#ChannelRegularConversion,NbrOfConversionFlag,ClockPrescaler,ContinuousConvMode,DMAContinuousRequests,Overrun,Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,OffsetNumber-2\#ChannelRegularConversion,Rank-3\#ChannelRegularConversion,Channel-3\#ChannelRegularConversion,SamplingTime-3\#ChannelRegularConversion,OffsetNumber-3\#ChannelRegularConversion,NbrOfConversion,ExternalTrigConv,Offset-3\#ChannelRegularConversion,EOCSelection,master,CommonPathInternal
ADC1.NbrOfConversion=3
ADC1.NbrOfConversionFlag=1
ADC1.Offset-3\#ChannelRegularConversion=2703
ADC1.OffsetNumber-1\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetNumber-2\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC1.OffsetNumber-3\#ChannelRegularConversion=ADC_OFFSET_1
ADC1.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC1.Rank-1\#ChannelRegularConversion=1
ADC1.Rank-2\#ChannelRegularConversion=2
ADC1.Rank-3\#ChannelRegularConversion=3
ADC1.SamplingTime-1\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.SamplingTime-3\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
ADC1.master=1
ADC2.Channel-1\#ChannelRegularConversion=ADC_CHANNEL_3
ADC2.Channel-2\#ChannelRegularConversion=ADC_CHANNEL_5
ADC2.ClockPrescaler=ADC_CLOCK_ASYNC_DIV4
ADC2.CommonPathInternal=null|null|null|null
ADC2.ContinuousConvMode=DISABLE
ADC2.DMAContinuousRequests=ENABLE
ADC2.EOCSelection=ADC_EOC_SEQ_CONV
ADC2.ExternalTrigConv=ADC_EXTERNALTRIG_HRTIM_TRG3
ADC2.IPParameters=Rank-1\#ChannelRegularConversion,Channel-1\#ChannelRegularConversion,SamplingTime-1\#ChannelRegularConversion,OffsetNumber-1\#ChannelRegularConversion,NbrOfConversionFlag,ClockPrescaler,NbrOfConversion,ContinuousConvMode,DMAContinuousRequests,Overrun,Rank-2\#ChannelRegularConversion,Channel-2\#ChannelRegularConversion,SamplingTime-2\#ChannelRegularConversion,OffsetNumber-2\#ChannelRegularConversion,ExternalTrigConv,EOCSelection,CommonPathInternal
ADC2.NbrOfConversion=2
ADC2.NbrOfConversionFlag=1
ADC2.OffsetNumber-1\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC2.OffsetNumber-2\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC2.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC2.Rank-1\#ChannelRegularConversion=1
ADC2.Rank-2\#ChannelRegularConversion=2
ADC2.SamplingTime-1\#ChannelRegularConversion=ADC_SAMPLETIME_6CYCLES_5
ADC2.SamplingTime-2\#ChannelRegularConversion=ADC_SAMPLETIME_47CYCLES_5
ADC3.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_1
ADC3.ClockPrescaler=ADC_CLOCK_ASYNC_DIV4
ADC3.CommonPathInternal=null|null|null|null
ADC3.ContinuousConvMode=DISABLE
ADC3.DMAContinuousRequests=ENABLE
ADC3.DataAlign=ADC_DATAALIGN_LEFT
ADC3.EOCSelection=ADC_EOC_SINGLE_CONV
ADC3.ExternalTrigConv=ADC_EXTERNALTRIG_HRTIM_TRG1
ADC3.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,master,ContinuousConvMode,NbrOfConversion,ExternalTrigConv,Overrun,ClockPrescaler,DMAContinuousRequests,Offset-0\#ChannelRegularConversion,OffsetSaturation-0\#ChannelRegularConversion,DataAlign,EOCSelection,CommonPathInternal
ADC3.NbrOfConversion=1
ADC3.NbrOfConversionFlag=1
ADC3.Offset-0\#ChannelRegularConversion=3208
ADC3.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_1
ADC3.OffsetSaturation-0\#ChannelRegularConversion=DISABLE
ADC3.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC3.Rank-0\#ChannelRegularConversion=1
ADC3.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_12CYCLES_5
ADC3.master=1
ADC4.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_3
ADC4.ClockPrescaler=ADC_CLOCK_ASYNC_DIV4
ADC4.CommonPathInternal=null|null|null|null
ADC4.ContinuousConvMode=ENABLE
ADC4.DMAContinuousRequests=ENABLE
ADC4.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,ClockPrescaler,ContinuousConvMode,DMAContinuousRequests,Overrun,CommonPathInternal
ADC4.NbrOfConversionFlag=1
ADC4.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC4.Overrun=ADC_OVR_DATA_OVERWRITTEN
ADC4.Rank-0\#ChannelRegularConversion=1
ADC4.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_47CYCLES_5
ADC5.Channel-0\#ChannelRegularConversion=ADC_CHANNEL_TEMPSENSOR_ADC5
ADC5.ClockPrescaler=ADC_CLOCK_ASYNC_DIV4
ADC5.CommonPathInternal=null|ADC_CHANNEL_TEMPSENSOR_ADC1|null|null
ADC5.ContinuousConvMode=ENABLE
ADC5.DMAContinuousRequests=ENABLE
ADC5.EOCSelection=ADC_EOC_SEQ_CONV
ADC5.ExternalTrigConv=ADC_SOFTWARE_START
ADC5.IPParameters=Rank-0\#ChannelRegularConversion,Channel-0\#ChannelRegularConversion,SamplingTime-0\#ChannelRegularConversion,OffsetNumber-0\#ChannelRegularConversion,NbrOfConversionFlag,DMAContinuousRequests,ContinuousConvMode,ExternalTrigConv,EOCSelection,ClockPrescaler,CommonPathInternal
ADC5.NbrOfConversionFlag=1
ADC5.OffsetNumber-0\#ChannelRegularConversion=ADC_OFFSET_NONE
ADC5.Rank-0\#ChannelRegularConversion=1
ADC5.SamplingTime-0\#ChannelRegularConversion=ADC_SAMPLETIME_247CYCLES_5
CAD.formats=
CAD.pinconfig=
CAD.provider=
COMP1.Hysteresis=COMP_HYSTERESIS_10MV
COMP1.IPParameters=TriggerMode,Hysteresis
COMP1.TriggerMode=COMP_TRIGGERMODE_IT_RISING
COMP3.Hysteresis=COMP_HYSTERESIS_10MV
COMP3.IPParameters=TriggerMode,Hysteresis
COMP3.TriggerMode=COMP_TRIGGERMODE_IT_RISING
COMP4.Hysteresis=COMP_HYSTERESIS_10MV
COMP4.IPParameters=TriggerMode,Hysteresis
COMP4.TriggerMode=COMP_TRIGGERMODE_IT_RISING
DAC1.DAC_DMADoubleDataMode-DAC_OUT1_Int=DISABLE
DAC1.DAC_Trigger_OUT1-DAC_OUT1_Int=DAC_TRIGGER_NONE
DAC1.IPParameters=DAC_Trigger_OUT1-DAC_OUT1_Int,DAC_DMADoubleDataMode-DAC_OUT1_Int
DAC3.DAC_Channel-DAC_OUT2_Int=DAC_CHANNEL_2
DAC3.IPParameters=DAC_Channel-DAC_OUT2_Int
Dma.ADC1.1.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC1.1.EventEnable=DISABLE
Dma.ADC1.1.Instance=DMA1_Channel2
Dma.ADC1.1.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC1.1.MemInc=DMA_MINC_ENABLE
Dma.ADC1.1.Mode=DMA_CIRCULAR
Dma.ADC1.1.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC1.1.PeriphInc=DMA_PINC_DISABLE
Dma.ADC1.1.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC1.1.Priority=DMA_PRIORITY_HIGH
Dma.ADC1.1.RequestNumber=1
Dma.ADC1.1.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC1.1.SignalID=NONE
Dma.ADC1.1.SyncEnable=DISABLE
Dma.ADC1.1.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC1.1.SyncRequestNumber=1
Dma.ADC1.1.SyncSignalID=NONE
Dma.ADC2.2.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC2.2.EventEnable=DISABLE
Dma.ADC2.2.Instance=DMA1_Channel3
Dma.ADC2.2.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC2.2.MemInc=DMA_MINC_ENABLE
Dma.ADC2.2.Mode=DMA_CIRCULAR
Dma.ADC2.2.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC2.2.PeriphInc=DMA_PINC_DISABLE
Dma.ADC2.2.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC2.2.Priority=DMA_PRIORITY_HIGH
Dma.ADC2.2.RequestNumber=1
Dma.ADC2.2.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC2.2.SignalID=NONE
Dma.ADC2.2.SyncEnable=DISABLE
Dma.ADC2.2.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC2.2.SyncRequestNumber=1
Dma.ADC2.2.SyncSignalID=NONE
Dma.ADC3.0.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC3.0.EventEnable=DISABLE
Dma.ADC3.0.Instance=DMA2_Channel1
Dma.ADC3.0.MemDataAlignment=DMA_MDATAALIGN_WORD
Dma.ADC3.0.MemInc=DMA_MINC_DISABLE
Dma.ADC3.0.Mode=DMA_CIRCULAR
Dma.ADC3.0.PeriphDataAlignment=DMA_PDATAALIGN_WORD
Dma.ADC3.0.PeriphInc=DMA_PINC_DISABLE
Dma.ADC3.0.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC3.0.Priority=DMA_PRIORITY_VERY_HIGH
Dma.ADC3.0.RequestNumber=1
Dma.ADC3.0.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC3.0.SignalID=NONE
Dma.ADC3.0.SyncEnable=DISABLE
Dma.ADC3.0.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC3.0.SyncRequestNumber=1
Dma.ADC3.0.SyncSignalID=NONE
Dma.ADC4.4.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC4.4.EventEnable=DISABLE
Dma.ADC4.4.Instance=DMA1_Channel1
Dma.ADC4.4.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC4.4.MemInc=DMA_MINC_DISABLE
Dma.ADC4.4.Mode=DMA_CIRCULAR
Dma.ADC4.4.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC4.4.PeriphInc=DMA_PINC_DISABLE
Dma.ADC4.4.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC4.4.Priority=DMA_PRIORITY_LOW
Dma.ADC4.4.RequestNumber=1
Dma.ADC4.4.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC4.4.SignalID=NONE
Dma.ADC4.4.SyncEnable=DISABLE
Dma.ADC4.4.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC4.4.SyncRequestNumber=1
Dma.ADC4.4.SyncSignalID=NONE
Dma.ADC5.3.Direction=DMA_PERIPH_TO_MEMORY
Dma.ADC5.3.EventEnable=DISABLE
Dma.ADC5.3.Instance=DMA1_Channel4
Dma.ADC5.3.MemDataAlignment=DMA_MDATAALIGN_HALFWORD
Dma.ADC5.3.MemInc=DMA_MINC_DISABLE
Dma.ADC5.3.Mode=DMA_CIRCULAR
Dma.ADC5.3.PeriphDataAlignment=DMA_PDATAALIGN_HALFWORD
Dma.ADC5.3.PeriphInc=DMA_PINC_DISABLE
Dma.ADC5.3.Polarity=HAL_DMAMUX_REQ_GEN_RISING
Dma.ADC5.3.Priority=DMA_PRIORITY_LOW
Dma.ADC5.3.RequestNumber=1
Dma.ADC5.3.RequestParameters=Instance,Direction,PeriphInc,MemInc,PeriphDataAlignment,MemDataAlignment,Mode,Priority,SignalID,Polarity,RequestNumber,SyncSignalID,SyncPolarity,SyncEnable,EventEnable,SyncRequestNumber
Dma.ADC5.3.SignalID=NONE
Dma.ADC5.3.SyncEnable=DISABLE
Dma.ADC5.3.SyncPolarity=HAL_DMAMUX_SYNC_NO_EVENT
Dma.ADC5.3.SyncRequestNumber=1
Dma.ADC5.3.SyncSignalID=NONE
Dma.Request0=ADC3
Dma.Request1=ADC1
Dma.Request2=ADC2
Dma.Request3=ADC5
Dma.Request4=ADC4
Dma.RequestsNb=5
FDCAN2.CalculateBaudRateNominal=3541666
FDCAN2.CalculateTimeBitNominal=282
FDCAN2.CalculateTimeQuantumNominal=94.11764705882354
FDCAN2.ExtFiltersNbr=2
FDCAN2.IPParameters=CalculateTimeQuantumNominal,CalculateTimeBitNominal,CalculateBaudRateNominal,StdFiltersNbr,ExtFiltersNbr
FDCAN2.StdFiltersNbr=0
File.Version=6
GPIO.groupedBy=Group By Peripherals
HRTIM1.ADCTrigger1_Source1=HRTIM_ADCTRIGGEREVENT13_MASTER_CMP2
HRTIM1.ADCTrigger3_Source1=HRTIM_ADCTRIGGEREVENT13_MASTER_CMP3
HRTIM1.ADCTrigger_Id1=HRTIM_ADCTRIGGER_1
HRTIM1.ADCTrigger_Id2=__NULL
HRTIM1.ADCTrigger_Id3=HRTIM_ADCTRIGGER_3
HRTIM1.Adrom_TE=HRTIM_TIM_ADROM_VALLEY
HRTIM1.Adrom_TF=HRTIM_TIM_ADROM_VALLEY
HRTIM1.Bmrom_TE=HRTIM_TIM_BMROM_VALLEY
HRTIM1.Bmrom_TF=HRTIM_TIM_BMROM_VALLEY
HRTIM1.CompareUnit1-MasterTimer=HRTIM_COMPAREUNIT_1
HRTIM1.CompareUnit1-Output_TE1TE2=HRTIM_COMPAREUNIT_1
HRTIM1.CompareUnit1-Output_TF1TF2=HRTIM_COMPAREUNIT_1
HRTIM1.CompareUnit2-MasterTimer=HRTIM_COMPAREUNIT_2
HRTIM1.CompareUnit3-MasterTimer=HRTIM_COMPAREUNIT_3
HRTIM1.CompareValue1-MasterTimer=6800
HRTIM1.CompareValue1-Output_TE1TE2=0
HRTIM1.CompareValue1-Output_TF1TF2=0
HRTIM1.CompareValue2-MasterTimer=6800
HRTIM1.CompareValue3-MasterTimer=10200
HRTIM1.DeadTimeInsertion-Output_TE1TE2=HRTIM_TIMDEADTIMEINSERTION_ENABLED
HRTIM1.DeadTimeInsertion-Output_TF1TF2=HRTIM_TIMDEADTIMEINSERTION_ENABLED
HRTIM1.Enable_FaultLine2=HRTIM_FAULTMODECTL_DISABLED
HRTIM1.Enable_FaultLine4=HRTIM_FAULTMODECTL_DISABLED
HRTIM1.Enable_FaultLine5=HRTIM_FAULTMODECTL_DISABLED
HRTIM1.Event_EEV1=__NULL
HRTIM1.FallingValue-Output_TE1TE2=15
HRTIM1.FallingValue-Output_TF1TF2=15
HRTIM1.Fault_Line1=__NULL
HRTIM1.Fault_Line2=HRTIM_FAULT_2
HRTIM1.Fault_Line4=HRTIM_FAULT_4
HRTIM1.Fault_Line5=HRTIM_FAULT_5
HRTIM1.Ferom_TE=HRTIM_TIM_FEROM_VALLEY
HRTIM1.Ferom_TF=HRTIM_TIM_FEROM_VALLEY
HRTIM1.GreaterCMP1_TE=HRTIM_TIMERGTCMP1_GREATER
HRTIM1.GreaterCMP1_TF=HRTIM_TIMERGTCMP1_GREATER
HRTIM1.IPParameters=Fault_Line1,Fault_Line2,Fault_Line4,Fault_Line5,PreloadEnable-Output_TE1TE2,CompareUnit1-Output_TE1TE2,GreaterCMP1_TE,UpDownMode-Output_TE1TE2,DeadTimeInsertion-Output_TE1TE2,UpDownMode-Output_TF1TF2,CompareUnit1-Output_TF1TF2,GreaterCMP1_TF,Ferom_TE,Bmrom_TE,Adrom_TE,Outrom_TE,rom_TE,Periode_TE,NumberUpdateTrigger-Output_TE1TE2,Periode_MASTER,PreloadEnable-MasterTimer,CompareUnit1-MasterTimer,InterleavedMode-MasterTimer,ResetUpdate-Output_TE1TE2,NumberResetTrigger-Output_TE1TE2,ResetTrigger1-Output_TE1TE2,CompareValue1-Output_TE1TE2,RisingValue-Output_TE1TE2,FallingValue-Output_TE1TE2,NumberSetSource1-Output_TE1TE2,SetOutput1_Source1-Output_TE1TE2,NumberSetSource2_TE,SetOutput2_Source1-Output_TE1TE2,Periode_TF,Ferom_TF,Bmrom_TF,Adrom_TF,Outrom_TF,rom_TF,PreloadEnable-Output_TF1TF2,DeadTimeInsertion-Output_TF1TF2,NumberUpdateTrigger-Output_TF1TF2,NumberResetTrigger-Output_TF1TF2,ResetTrigger1-Output_TF1TF2,CompareValue1-Output_TF1TF2,RisingValue-Output_TF1TF2,FallingValue-Output_TF1TF2,NumberSetSource1-Output_TF1TF2,SetOutput1_Source1-Output_TF1TF2,NumberSetSource2_TF,SetOutput2_Source1-Output_TF1TF2,ADCTrigger_Id1,Event_EEV1,CompareUnit2-MasterTimer,SyncOptions,Enable_FaultLine2,Enable_FaultLine4,Enable_FaultLine5,RepetitionUpdate-MasterTimer,ModeTimeBase-MasterTimer,ADCTrigger_Id2,NumberADCTriggerSource1,ADCTrigger1_Source1,ResetUpdate-Output_TF1TF2,RepetitionUpdate-Output_TE1TE2,UpdateTrigger1-Output_TE1TE2,RepetitionUpdate-Output_TF1TF2,UpdateTrigger1-Output_TF1TF2,CompareValue1-MasterTimer,CompareValue2-MasterTimer,CompareUnit3-MasterTimer,CompareValue3-MasterTimer,ADCTrigger_Id3,NumberADCTriggerSource3,ADCTrigger3_Source1
HRTIM1.InterleavedMode-MasterTimer=HRTIM_INTERLEAVED_MODE_DISABLED
HRTIM1.ModeTimeBase-MasterTimer=HRTIM_MODE_CONTINUOUS
HRTIM1.NumberADCTriggerSource1=1
HRTIM1.NumberADCTriggerSource3=1
HRTIM1.NumberResetTrigger-Output_TE1TE2=1
HRTIM1.NumberResetTrigger-Output_TF1TF2=1
HRTIM1.NumberSetSource1-Output_TE1TE2=1
HRTIM1.NumberSetSource1-Output_TF1TF2=1
HRTIM1.NumberSetSource2_TE=1
HRTIM1.NumberSetSource2_TF=1
HRTIM1.NumberUpdateTrigger-Output_TE1TE2=1
HRTIM1.NumberUpdateTrigger-Output_TF1TF2=1
HRTIM1.Outrom_TE=HRTIM_TIM_OUTROM_VALLEY
HRTIM1.Outrom_TF=HRTIM_TIM_OUTROM_VALLEY
HRTIM1.Periode_MASTER=13600
HRTIM1.Periode_TE=6800
HRTIM1.Periode_TF=6800
HRTIM1.PreloadEnable-MasterTimer=HRTIM_PRELOAD_ENABLED
HRTIM1.PreloadEnable-Output_TE1TE2=HRTIM_PRELOAD_ENABLED
HRTIM1.PreloadEnable-Output_TF1TF2=HRTIM_PRELOAD_ENABLED
HRTIM1.RepetitionUpdate-MasterTimer=HRTIM_UPDATEONREPETITION_ENABLED
HRTIM1.RepetitionUpdate-Output_TE1TE2=HRTIM_UPDATEONREPETITION_ENABLED
HRTIM1.RepetitionUpdate-Output_TF1TF2=HRTIM_UPDATEONREPETITION_ENABLED
HRTIM1.ResetTrigger1-Output_TE1TE2=HRTIM_TIMRESETTRIGGER_MASTER_CMP1
HRTIM1.ResetTrigger1-Output_TF1TF2=HRTIM_TIMRESETTRIGGER_MASTER_PER
HRTIM1.ResetUpdate-Output_TE1TE2=HRTIM_TIMUPDATEONRESET_ENABLED
HRTIM1.ResetUpdate-Output_TF1TF2=HRTIM_TIMUPDATEONRESET_ENABLED
HRTIM1.RisingValue-Output_TE1TE2=15
HRTIM1.RisingValue-Output_TF1TF2=15
HRTIM1.SetOutput1_Source1-Output_TE1TE2=HRTIM_OUTPUTSET_TIMCMP1
HRTIM1.SetOutput1_Source1-Output_TF1TF2=HRTIM_OUTPUTSET_TIMCMP1
HRTIM1.SetOutput2_Source1-Output_TE1TE2=HRTIM_OUTPUTSET_TIMCMP1
HRTIM1.SetOutput2_Source1-Output_TF1TF2=HRTIM_OUTPUTSET_TIMCMP1
HRTIM1.SyncOptions=HRTIM_SYNCOPTION_NONE
HRTIM1.UpDownMode-Output_TE1TE2=HRTIM_TIMERUPDOWNMODE_UPDOWN
HRTIM1.UpDownMode-Output_TF1TF2=HRTIM_TIMERUPDOWNMODE_UPDOWN
HRTIM1.UpdateTrigger1-Output_TE1TE2=HRTIM_TIMUPDATETRIGGER_TIMER_E
HRTIM1.UpdateTrigger1-Output_TF1TF2=HRTIM_TIMUPDATETRIGGER_TIMER_F
HRTIM1.rom_TE=HRTIM_TIM_ROM_VALLEY
HRTIM1.rom_TF=HRTIM_TIM_ROM_VALLEY
I2C1.IPParameters=Timing
I2C1.Timing=0x40B285C2
KeepUserPlacement=false
Mcu.CPN=STM32G474RBT6
Mcu.Family=STM32G4
Mcu.IP0=ADC1
Mcu.IP1=ADC2
Mcu.IP10=DMA
Mcu.IP11=FDCAN2
Mcu.IP12=FMAC
Mcu.IP13=HRTIM1
Mcu.IP14=I2C1
Mcu.IP15=NVIC
Mcu.IP16=OPAMP1
Mcu.IP17=OPAMP2
Mcu.IP18=RCC
Mcu.IP19=SYS
Mcu.IP2=ADC3
Mcu.IP20=TIM1
Mcu.IP21=TIM6
Mcu.IP22=TIM7
Mcu.IP23=TIM16
Mcu.IP24=UART4
Mcu.IP3=ADC4
Mcu.IP4=ADC5
Mcu.IP5=COMP1
Mcu.IP6=COMP3
Mcu.IP7=COMP4
Mcu.IP8=DAC1
Mcu.IP9=DAC3
Mcu.IPNb=25
Mcu.Name=STM32G474R(B-C-E)Tx
Mcu.Package=LQFP64
Mcu.Pin0=PC13
Mcu.Pin1=PF0-OSC_IN
Mcu.Pin10=PA5
Mcu.Pin11=PA6
Mcu.Pin12=PA7
Mcu.Pin13=PC4
Mcu.Pin14=PC5
Mcu.Pin15=PB0
Mcu.Pin16=PB1
Mcu.Pin17=VREF+
Mcu.Pin18=PB10
Mcu.Pin19=PB12
Mcu.Pin2=PF1-OSC_OUT
Mcu.Pin20=PB13
Mcu.Pin21=PC6
Mcu.Pin22=PC7
Mcu.Pin23=PC8
Mcu.Pin24=PC9
Mcu.Pin25=PA9
Mcu.Pin26=PA13
Mcu.Pin27=PA14
Mcu.Pin28=PC10
Mcu.Pin29=PC11
Mcu.Pin3=PG10-NRST
Mcu.Pin30=PC12
Mcu.Pin31=PD2
Mcu.Pin32=PB3
Mcu.Pin33=PB4
Mcu.Pin34=PB5
Mcu.Pin35=PB6
Mcu.Pin36=PB7
Mcu.Pin37=PB8-BOOT0
Mcu.Pin38=PB9
Mcu.Pin39=VP_ADC5_TempSens_Input
Mcu.Pin4=PC0
Mcu.Pin40=VP_COMP1_VS_DAC1OUT1
Mcu.Pin41=VP_COMP3_VS_DAC3OUT1
Mcu.Pin42=VP_COMP4_VS_DAC3OUT2
Mcu.Pin43=VP_DAC1_VS_DACI1
Mcu.Pin44=VP_DAC3_VS_DACI1
Mcu.Pin45=VP_DAC3_VS_DACI2
Mcu.Pin46=VP_FMAC_VS_FMAC
Mcu.Pin47=VP_HRTIM1_VS_hrtimMasterTimerNoOutput
Mcu.Pin48=VP_SYS_VS_Systick
Mcu.Pin49=VP_SYS_VS_DBSignals
Mcu.Pin5=PC1
Mcu.Pin50=VP_TIM1_VS_ClockSourceINT
Mcu.Pin51=VP_TIM6_VS_ClockSourceINT
Mcu.Pin52=VP_TIM7_VS_ClockSourceINT
Mcu.Pin53=VP_TIM16_VS_ClockSourceINT
Mcu.Pin6=PC2
Mcu.Pin7=PA1
Mcu.Pin8=PA2
Mcu.Pin9=PA3
Mcu.PinsNb=54
Mcu.ThirdPartyNb=0
Mcu.UserConstants=
Mcu.UserName=STM32G474RBTx
MxCube.Version=6.15.0
MxDb.Version=DB.6.0.150
NVIC.BusFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.COMP1_2_3_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true
NVIC.COMP4_5_6_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:true
NVIC.DebugMonitor_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.FDCAN2_IT0_IRQn=true\:15\:0\:true\:false\:true\:true\:true\:true
NVIC.FDCAN2_IT1_IRQn=true\:1\:0\:true\:false\:true\:true\:true\:true
NVIC.FMAC_IRQn=true\:0\:0\:true\:false\:true\:true\:true\:true
NVIC.ForceEnableDMAVector=false
NVIC.HRTIM1_FLT_IRQn=true\:1\:0\:true\:false\:true\:true\:true\:true
NVIC.HardFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.MemoryManagement_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.NonMaskableInt_IRQn=true\:0\:0\:false\:false\:true\:false\:true\:false
NVIC.PendSV_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.PriorityGroup=NVIC_PRIORITYGROUP_4
NVIC.SVCall_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
NVIC.SysTick_IRQn=true\:2\:0\:true\:false\:true\:false\:true\:false
NVIC.TIM1_UP_TIM16_IRQn=true\:1\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM6_DAC_IRQn=true\:2\:0\:true\:false\:true\:true\:true\:true
NVIC.TIM7_DAC_IRQn=true\:3\:0\:true\:false\:true\:true\:true\:true
NVIC.UART4_IRQn=true\:3\:0\:true\:false\:true\:true\:true\:true
NVIC.UsageFault_IRQn=true\:0\:0\:false\:false\:true\:false\:false\:false
OPAMP1.IPParameters=PowerMode
OPAMP1.PowerMode=OPAMP_POWERMODE_HIGHSPEED
OPAMP2.IPParameters=PowerMode
OPAMP2.PowerMode=OPAMP_POWERMODE_HIGHSPEED
PA1.GPIOParameters=GPIO_Label
PA1.GPIO_Label=TEMP_OP+
PA1.Locked=true
PA1.Mode=Standalone
PA1.Signal=OPAMP1_VINP
PA13.Locked=true
PA13.Mode=Trace_Asynchronous_SW
PA13.Signal=SYS_JTMS-SWDIO
PA14.Locked=true
PA14.Mode=Trace_Asynchronous_SW
PA14.Signal=SYS_JTCK-SWCLK
PA2.GPIOParameters=GPIO_Label
PA2.GPIO_Label=TEMP_OUT_ADC
PA2.Locked=true
PA2.Signal=SharedAnalog_PA2
PA3.GPIOParameters=GPIO_Label
PA3.GPIO_Label=TEMP_OP-
PA3.Locked=true
PA3.Mode=Standalone
PA3.Signal=OPAMP1_VINM
PA5.GPIOParameters=GPIO_Label
PA5.GPIO_Label=VFLY_OP-
PA5.Locked=true
PA5.Mode=Standalone
PA5.Signal=OPAMP2_VINM
PA6.GPIOParameters=GPIO_Label
PA6.GPIO_Label=VFLY_OUT_ADC
PA6.Locked=true
PA6.Signal=SharedAnalog_PA6
PA7.GPIOParameters=GPIO_Label
PA7.GPIO_Label=VFLY_OP+
PA7.Locked=true
PA7.Mode=Standalone
PA7.Signal=OPAMP2_VINP
PA9.Locked=true
PA9.Mode=IN2-Single-Ended
PA9.Signal=ADC5_IN2
PB0.GPIOParameters=GPIO_Label
PB0.GPIO_Label=I_LOAD_COMP
PB0.Locked=true
PB0.Mode=INP
PB0.Signal=COMP4_INP
PB1.GPIOParameters=GPIO_Label
PB1.GPIO_Label=V_OUT_COMP_ADC3
PB1.Locked=true
PB1.Signal=SharedAnalog_PB1
PB10.GPIOParameters=GPIO_Label
PB10.GPIO_Label=DISCONNECT_OUTPUT
PB10.Locked=true
PB10.Signal=GPIO_Output
PB12.GPIOParameters=GPIO_Label
PB12.GPIO_Label=VBAT_ADC
PB12.Locked=true
PB12.Mode=IN3-Single-Ended
PB12.Signal=ADC4_IN3
PB13.GPIOParameters=GPIO_Label
PB13.GPIO_Label=ENABLE_ISO_FET
PB13.Locked=true
PB13.Signal=GPIO_Output
PB3.Locked=true
PB3.Mode=Trace_Asynchronous_SW
PB3.Signal=SYS_JTDO-SWO
PB4.GPIOParameters=GPIO_Label
PB4.GPIO_Label=PRECHARGE
PB4.Locked=true
PB4.Signal=GPIO_Output
PB5.Locked=true
PB5.Mode=FDCAN_Activate
PB5.Signal=FDCAN2_RX
PB6.Locked=true
PB6.Mode=FDCAN_Activate
PB6.Signal=FDCAN2_TX
PB7.Locked=true
PB7.Mode=I2C
PB7.Signal=I2C1_SDA
PB8-BOOT0.Locked=true
PB8-BOOT0.Mode=I2C
PB8-BOOT0.Signal=I2C1_SCL
PB9.GPIOParameters=GPIO_Label
PB9.GPIO_Label=DISCONNECT_INPUT
PB9.Locked=true
PB9.Signal=GPIO_Output
PC0.GPIOParameters=GPIO_Label
PC0.GPIO_Label=V_IN_ADC
PC0.Locked=true
PC0.Mode=IN6-Single-Ended
PC0.Signal=ADC1_IN6
PC1.GPIOParameters=GPIO_Label
PC1.GPIO_Label=I_IN_COMP_ADC
PC1.Locked=true
PC1.Signal=SharedAnalog_PC1
PC10.GPIOParameters=GPIO_Label
PC10.GPIO_Label=VCP_TX
PC10.Locked=true
PC10.Mode=Asynchronous
PC10.Signal=UART4_TX
PC11.GPIOParameters=GPIO_Label
PC11.GPIO_Label=VCP_RX
PC11.Locked=true
PC11.Mode=Asynchronous
PC11.Signal=UART4_RX
PC12.Locked=true
PC12.Signal=GPIO_Output
PC13.GPIOParameters=GPIO_Label
PC13.GPIO_Label=ALARM
PC13.Locked=true
PC13.Mode=PWM Generation1 CH1N
PC13.Signal=TIM1_CH1N
PC2.GPIOParameters=GPIO_Label
PC2.GPIO_Label=NTC_BOARD
PC2.Locked=true
PC2.Mode=IN8-Single-Ended
PC2.Signal=ADC1_IN8
PC4.GPIOParameters=GPIO_Label
PC4.GPIO_Label=I_LOAD_ADC
PC4.Locked=true
PC4.Mode=IN5-Single-Ended
PC4.Signal=ADC2_IN5
PC5.GPIOParameters=GPIO_Label
PC5.GPIO_Label=TEST_PC5
PC5.Locked=true
PC5.Signal=GPIO_Output
PC6.GPIOParameters=GPIO_Label
PC6.GPIO_Label=PWM4
PC6.Locked=true
PC6.Mode=Output_TF1TF2
PC6.Signal=HRTIM1_CHF1
PC7.GPIOParameters=GPIO_Label
PC7.GPIO_Label=PWM1
PC7.Locked=true
PC7.Mode=Output_TF1TF2
PC7.Signal=HRTIM1_CHF2
PC8.GPIOParameters=GPIO_Label
PC8.GPIO_Label=PWM3
PC8.Locked=true
PC8.Mode=Output_TE1TE2
PC8.Signal=HRTIM1_CHE1
PC9.GPIOParameters=GPIO_Label
PC9.GPIO_Label=PWM2
PC9.Locked=true
PC9.Mode=Output_TE1TE2
PC9.Signal=HRTIM1_CHE2
PD2.GPIOParameters=GPIO_Label
PD2.GPIO_Label=FDCAN_SILENT
PD2.Locked=true
PD2.Signal=GPIO_Output
PF0-OSC_IN.Locked=true
PF0-OSC_IN.Mode=HSE-External-Oscillator
PF0-OSC_IN.Signal=RCC_OSC_IN
PF1-OSC_OUT.Locked=true
PF1-OSC_OUT.Mode=HSE-External-Oscillator
PF1-OSC_OUT.Signal=RCC_OSC_OUT
PG10-NRST.Locked=true
PinOutPanel.RotationAngle=0
ProjectManager.AskForMigrate=true
ProjectManager.BackupPrevious=false
ProjectManager.CompilerLinker=GCC
ProjectManager.CompilerOptimize=6
ProjectManager.ComputerToolchain=false
ProjectManager.CoupleFile=false
ProjectManager.CustomerFirmwarePackage=
ProjectManager.DefaultFWLocation=true
ProjectManager.DeletePrevious=true
ProjectManager.DeviceId=STM32G474RBTx
ProjectManager.FirmwarePackage=STM32Cube FW_G4 V1.6.1
ProjectManager.FreePins=false
ProjectManager.HalAssertFull=false
ProjectManager.HeapSize=0x200
ProjectManager.KeepUserCode=true
ProjectManager.LastFirmware=false
ProjectManager.LibraryCopy=1
ProjectManager.MainLocation=Core/Src
ProjectManager.NoMain=false
ProjectManager.PreviousToolchain=STM32CubeIDE
ProjectManager.ProjectBuild=false
ProjectManager.ProjectFileName=LVSolarBuck64.ioc
ProjectManager.ProjectName=LVSolarBuck64
ProjectManager.ProjectStructure=
ProjectManager.RegisterCallBack=
ProjectManager.StackSize=0x400
ProjectManager.TargetToolchain=STM32CubeIDE
ProjectManager.ToolChainLocation=
ProjectManager.UAScriptAfterPath=
ProjectManager.UAScriptBeforePath=
ProjectManager.UnderRoot=true
ProjectManager.functionlistsort=1-SystemClock_Config-RCC-false-HAL-false,2-MX_GPIO_Init-GPIO-false-HAL-true,3-MX_DMA_Init-DMA-false-HAL-true,4-MX_ADC3_Init-ADC3-false-HAL-true,5-MX_ADC5_Init-ADC5-false-HAL-true,6-MX_FDCAN2_Init-FDCAN2-false-HAL-true,7-MX_HRTIM1_Init-HRTIM1-false-HAL-true,8-MX_I2C1_Init-I2C1-false-HAL-true,9-MX_UART4_Init-UART4-false-HAL-true,10-MX_ADC1_Init-ADC1-false-HAL-true,11-MX_ADC2_Init-ADC2-false-HAL-true,12-MX_OPAMP2_Init-OPAMP2-false-HAL-true,13-MX_COMP1_Init-COMP1-false-HAL-true,14-MX_COMP3_Init-COMP3-false-HAL-true,15-MX_COMP4_Init-COMP4-false-HAL-true,16-MX_DAC1_Init-DAC1-false-HAL-true,17-MX_DAC3_Init-DAC3-false-HAL-true,18-MX_OPAMP1_Init-OPAMP1-false-HAL-true,19-MX_TIM1_Init-TIM1-false-HAL-true,20-MX_FMAC_Init-FMAC-false-HAL-true,21-MX_TIM6_Init-TIM6-false-HAL-true,22-MX_TIM7_Init-TIM7-false-HAL-true,23-MX_TIM16_Init-TIM16-false-HAL-true,24-MX_ADC4_Init-ADC4-false-HAL-true
RCC.ADC12Freq_Value=170000000
RCC.ADC345Freq_Value=170000000
RCC.AHBFreq_Value=170000000
RCC.APB1Freq_Value=170000000
RCC.APB1TimFreq_Value=170000000
RCC.APB2Freq_Value=170000000
RCC.APB2TimFreq_Value=170000000
RCC.CRSFreq_Value=48000000
RCC.CortexFreq_Value=21250000
RCC.Cortex_Div=SYSTICK_CLKSOURCE_HCLK_DIV8
RCC.EXTERNAL_CLOCK_VALUE=12288000
RCC.EnbaleCSS=true
RCC.FCLKCortexFreq_Value=170000000
RCC.FDCANFreq_Value=170000000
RCC.FamilyName=M
RCC.HCLKFreq_Value=170000000
RCC.HRTIM1Freq_Value=170000000
RCC.HSE_VALUE=40000000
RCC.HSI48_VALUE=48000000
RCC.HSI_VALUE=16000000
RCC.I2C1Freq_Value=170000000
RCC.I2C2Freq_Value=170000000
RCC.I2C3Freq_Value=170000000
RCC.I2C4Freq_Value=170000000
RCC.I2SFreq_Value=170000000
RCC.IPParameters=ADC12Freq_Value,ADC345Freq_Value,AHBFreq_Value,APB1Freq_Value,APB1TimFreq_Value,APB2Freq_Value,APB2TimFreq_Value,CRSFreq_Value,CortexFreq_Value,Cortex_Div,EXTERNAL_CLOCK_VALUE,EnbaleCSS,FCLKCortexFreq_Value,FDCANFreq_Value,FamilyName,HCLKFreq_Value,HRTIM1Freq_Value,HSE_VALUE,HSI48_VALUE,HSI_VALUE,I2C1Freq_Value,I2C2Freq_Value,I2C3Freq_Value,I2C4Freq_Value,I2SFreq_Value,LPTIM1Freq_Value,LPUART1Freq_Value,LSCOPinFreq_Value,LSE_VALUE,LSI_VALUE,MCO1PinFreq_Value,PLLM,PLLN,PLLP,PLLPoutputFreq_Value,PLLQoutputFreq_Value,PLLRCLKFreq_Value,PLLSourceVirtual,PWRFreq_Value,QSPIFreq_Value,RNGFreq_Value,SAI1Freq_Value,SYSCLKFreq_VALUE,SYSCLKSource,UART4Freq_Value,UART5Freq_Value,USART1Freq_Value,USART2Freq_Value,USART3Freq_Value,USBFreq_Value,VCOInputFreq_Value,VCOOutputFreq_Value
RCC.LPTIM1Freq_Value=170000000
RCC.LPUART1Freq_Value=170000000
RCC.LSCOPinFreq_Value=32000
RCC.LSE_VALUE=32768
RCC.LSI_VALUE=32000
RCC.LockedElements=AHBOutput
RCC.MCO1PinFreq_Value=16000000
RCC.PLLM=RCC_PLLM_DIV4
RCC.PLLN=34
RCC.PLLP=RCC_PLLP_DIV4
RCC.PLLPoutputFreq_Value=85000000
RCC.PLLQoutputFreq_Value=170000000
RCC.PLLRCLKFreq_Value=170000000
RCC.PLLSourceVirtual=RCC_PLLSOURCE_HSE
RCC.PWRFreq_Value=170000000
RCC.QSPIFreq_Value=170000000
RCC.RNGFreq_Value=170000000
RCC.SAI1Freq_Value=170000000
RCC.SYSCLKFreq_VALUE=170000000
RCC.SYSCLKSource=RCC_SYSCLKSOURCE_PLLCLK
RCC.UART4Freq_Value=170000000
RCC.UART5Freq_Value=170000000
RCC.USART1Freq_Value=170000000
RCC.USART2Freq_Value=170000000
RCC.USART3Freq_Value=170000000
RCC.USBFreq_Value=170000000
RCC.VCOInputFreq_Value=10000000
RCC.VCOOutputFreq_Value=340000000
SH.SharedAnalog_PA2.0=OPAMP1_VOUT,Standalone
SH.SharedAnalog_PA2.1=ADC1_IN3,IN3-Single-Ended
SH.SharedAnalog_PA2.ConfNb=2
SH.SharedAnalog_PA6.0=ADC2_IN3,IN3-Single-Ended
SH.SharedAnalog_PA6.1=OPAMP2_VOUT,Standalone
SH.SharedAnalog_PA6.ConfNb=2
SH.SharedAnalog_PB1.0=ADC3_IN1,IN1-Single-Ended
SH.SharedAnalog_PB1.1=COMP1_INP,INP
SH.SharedAnalog_PB1.ConfNb=2
SH.SharedAnalog_PC1.0=COMP3_INP,INP
SH.SharedAnalog_PC1.1=ADC1_IN7,IN7-Single-Ended
SH.SharedAnalog_PC1.ConfNb=2
SYS.IPParameters=VoltageScaling
SYS.VoltageScaling=SYSCFG_VREFBUF_VOLTAGE_SCALE1
TIM1.Channel-PWM\ Generation1\ CH1N=TIM_CHANNEL_1
TIM1.IPParameters=Channel-PWM Generation1 CH1N,PeriodNoDither,Prescaler,PulseNoDither_1,OCFastMode_PWM-PWM Generation1 CH1N
TIM1.OCFastMode_PWM-PWM\ Generation1\ CH1N=TIM_OCFAST_ENABLE
TIM1.PeriodNoDither=3542
TIM1.Prescaler=20-1
TIM1.PulseNoDither_1=1771
TIM16.IPParameters=Prescaler,PeriodNoDither
TIM16.PeriodNoDither=20
TIM16.Prescaler=170-1
TIM6.IPParameters=Prescaler,PeriodNoDither
TIM6.PeriodNoDither=100
TIM6.Prescaler=1700-1
TIM7.IPParameters=Prescaler,PeriodNoDither
TIM7.PeriodNoDither=5000
TIM7.Prescaler=3400-1
UART4.BaudRate=460800
UART4.IPParameters=Mode,BaudRate
UART4.Mode=MODE_TX_RX
VP_ADC5_TempSens_Input.Mode=IN-TempSens
VP_ADC5_TempSens_Input.Signal=ADC5_TempSens_Input
VP_COMP1_VS_DAC1OUT1.Mode=INM_DAC1OUT1
VP_COMP1_VS_DAC1OUT1.Signal=COMP1_VS_DAC1OUT1
VP_COMP3_VS_DAC3OUT1.Mode=INM_DAC3OUT1
VP_COMP3_VS_DAC3OUT1.Signal=COMP3_VS_DAC3OUT1
VP_COMP4_VS_DAC3OUT2.Mode=INM_DAC3OUT2
VP_COMP4_VS_DAC3OUT2.Signal=COMP4_VS_DAC3OUT2
VP_DAC1_VS_DACI1.Mode=DAC_OUT1_Int
VP_DAC1_VS_DACI1.Signal=DAC1_VS_DACI1
VP_DAC3_VS_DACI1.Mode=DAC_OUT1_Int
VP_DAC3_VS_DACI1.Signal=DAC3_VS_DACI1
VP_DAC3_VS_DACI2.Mode=DAC_OUT2_Int
VP_DAC3_VS_DACI2.Signal=DAC3_VS_DACI2
VP_FMAC_VS_FMAC.Mode=FMAC_Activate
VP_FMAC_VS_FMAC.Signal=FMAC_VS_FMAC
VP_HRTIM1_VS_hrtimMasterTimerNoOutput.Mode=MasterTimer
VP_HRTIM1_VS_hrtimMasterTimerNoOutput.Signal=HRTIM1_VS_hrtimMasterTimerNoOutput
VP_SYS_VS_DBSignals.Mode=DisableDeadBatterySignals
VP_SYS_VS_DBSignals.Signal=SYS_VS_DBSignals
VP_SYS_VS_Systick.Mode=SysTick
VP_SYS_VS_Systick.Signal=SYS_VS_Systick
VP_TIM16_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM16_VS_ClockSourceINT.Signal=TIM16_VS_ClockSourceINT
VP_TIM1_VS_ClockSourceINT.Mode=Internal
VP_TIM1_VS_ClockSourceINT.Signal=TIM1_VS_ClockSourceINT
VP_TIM6_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM6_VS_ClockSourceINT.Signal=TIM6_VS_ClockSourceINT
VP_TIM7_VS_ClockSourceINT.Mode=Enable_Timer
VP_TIM7_VS_ClockSourceINT.Signal=TIM7_VS_ClockSourceINT
VREF+.Locked=true
VREF+.Mode=InternalMode
VREF+.Signal=VREFBUF_OUT
board=custom
